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Specifications for Architects, Engineers and Specifiers
Arithmetic Design, Inc.
ABSORB Pure Acoustic Absorber Panels

Section 09 84 5


NOTE TO ARCHITECT: This guide specification was prepared by Arithmetic Design, Inc. in accordance with CSI standards and formats.  This section includes specification for ABSORB acoustic absorber panels and appropriate mounting practice. This section must be carefully examined, reviewed and edited by the Architect to meet project requirements and local building codes.  Coordinate this section with other specification sections and project drawings.

NOTE TO SPECIFIER:  This section covers Arithmetic Design ABSORB Pure acoustic panels in polyester recycled material. 

NOTE TO SPECIFIER:  This section should be modified to suit project requirements. Modify or add items as necessary. Delete items which are not applicable. Words and sentences within bold brackets [____ ] reflect a choice to be made with regard to an item or statement. Please contact Arithmetic Design for updates and revisions to this section.  



PART 1: GENERAL

	1.01 SECTION INCLUDES

		A.  ABSORB Pure acoustic absorber panels
		B.  Coordination of trades associated with installation and implementation of acoustical panels described in this section.

	1.02  RELATED PRODUCTS NOT SPECIFIED IN THIS SECTION

		A. 	Section 09120 – Suspension Framing/Furring for Plaster/Gypsum Board Assemblies
B.	Section 09200 – Plaster & Gypsum Board
C.	Section 09500 – Acoustic Tile Ceilings: Suspension Systems
D.	Div 15 Section – Mechanical
E.	Div 16 Section – Electrical
F.	Div 17 Section – Audio, Data, Telecommunication

	1.04  ALTERNATES

		A.  Proposed substitutions for products in this section must be submitted to acoustic consultant and architect. Submissions 			      for substitutions must be in accordance with due dates determined by General Contractor.  Substitutions shall only be 			      considered when appropriate acoustic data and tangible sample showing design, composition and finish.

	1.05  REFERENCES

(Note to Specifier: modify section as necessary.) 

		A.  Local Building Code - Current Edition
		B.  Industry Standard Test Methods
		1.  ISO 354 Measurement of Sound Absorption in a Reverberation Room
2.  ISO 10534 - Determination of sound absorption coefficient and impedance
3.  ASTM E 1050-98 - Standard Test Method for Impedance and Absorption of Acoustical Materials Using a Tube, Two Microphones, and a Digital Frequency Analysis System
4.  ASTM C 423 - Sound Absorption & Sound Absorption Coefficients by the Reverberation Room Method

	


1.06  DESIGN REQUIREMENTS

(Note to Specifier: modify section as necessary.) 

		A.  Provide wide bandwidth acoustic absorption with a 7 pcf polyester core.
		B.  Flat or shaped polyester absorber design elements

	1.07  PERFORMANCE REQUIREMENTS

(Note to Specifier: modify section as necessary.) 

		A.  Sound absorption 
		B.  Performance verified by accredited NVLAP facility under ASTM C423-a industry standard test methods

	1.08  SUBMITTALS

		A.  Submit in accordance with provisions of Section 01300
		B.  Product Data: Submit manufacturers installation instructions and technical data including descriptions and sizes certifying  		      conformance with specified performance requirements. Include pertinent size, spacing and dimensional data. 
		C.  Shop drawings: Submit shop drawings of products, mountings and installation instructions. Show details of interior 			      renderings including dimensions, orientation and location of any element that may interfere with the installation and 			      integration. Indicate standoff lengths of individual panels. Indicate hole patterns and panel spacing requirements on shop  		      drawings. Verify site dimensional accuracy per shop drawings.
		D.  Samples: Submit individual product sample including standoffs demonstrating size, composition and specified finish.

	1.09  QUALITY ASSURANCE

		A.  Produce Source: Products under this section shall be supplied from a single manufacturer to ensure consistency of 			      performance, size and finish.
		B.  Installer Qualifications: Installer shall have prior experience in working with similar products including handling, receiving 		      and inspecting similar products with verified minimum experience of (2) years. 

	1.10  DELIVERY, STORAGE AND HANDLING

		A.  Delivery and Receiving: Products shall be delivered and received in manufacturers original and unopened packaging. 			      Packaging shall be inspected for damage and proper conditions. Damage shall be reported to superintendent, carrier or 			      manufacturer. Carrier must be notified of unsatisfactory product conditions upon receipt if damage is present. Products shall 		      not be unpackaged until required environment and site conditions are present for installation. 
		B.  Storage: Products shall be stored in a clean, dry and enclosed facility. Moisture conditions should be minimal or as required 		      to prevent absorption of moisture and resultant warping and disfigurement of wood products.
		C.  Acceptance and Installation: Partial or full installation denotes full acceptance of product delivery. 
		D.  Disposal and Waste: All packaging, waste and refuse shall be disposed of in a responsible manner in accordance with 			      General Contractors policies and procedures and/or as site facilities allow. When disposing of materials, consider recycling 		      when provided on site. All disposal must be in accordance with local ordinance and in accordance with applicable regulating 		      bodies.
		E.  Environmental: Installation of products shall not commence until building and site has been appropriately enclosed and 			      acceptable interior environment conditions exist. Allow a minimum of (48) hours for humidity and temperature conditions 		      to stabilize before installation. 
		F.  Installation inspection: Allow (24) hours following installation to inspect torque and alignment of all mounting and anchoring 		      devices. If torque is not appropriate to bear panel weight, make necessary adjustments.  Standoff and anchors are required to 		      be solid and should not rattle.  Take appropriate actions to ensure solid anchors.


PART 2: PRODUCTS

	2.01  MANUFACTURER

		A.  Arithmetic Design, Inc., P.O. Box 11074, Denver, CO 80211, (720) 255-1604; www.arithmetic-design.com
		B.  Substitutions and alternates must be approved as noted above or in accordance with General Contractor's addendum.

	2.02  MATERIALS

		A.  Wrapped fiberglass Class A 
			1.  1" thickness: NRC: 0.70
			2.  2" thickness: NRC: 1.05
		B.  Designer/Architect specified finish.
		C.  Standard finish with color specification

	2.03  MANUFACTURED UNITS

(Note to Specifier: modify section as necessary.) 
		
		A. Sizes specification
			1.  [2' height x 2' width x 1" depth (nominal)]
			2.  [2' height x 4' width x 1" depth (nominal)]
			3.  [4' height x 4' width x 1" depth (nominal)] 
			4.  [4' height x 8' width x 1" depth (nominal)]
		B.  Finished unit dimensions (as manufactured)
			1.  [(2' x 2') - 23.750" x 23.750" x 1"]
			2.  [(2' x 4') - 23.750" x 47.750" x 1"]
			3.  [(4' x 4') - 47.750" x 47.750" x 1"]
			4.  [(4' x 8') - 47.750" x 95.750" x 1"]
	

	2.04  MOUNTING

(Note to Specifier: modify section as necessary.) 

		A.  Hardware options:
			1.  Impaling clips
			2.  Z-clips (resin hardening required)
			3.  Adhesive & impaling clips
	

PART 3: EXECUTION

	3.01 EXAMINATION

		A.  Examine products in this section for manufacturer specified sizes and finish. Do not proceed with product installation until 		      satisfactory working conditions are present. If satisfactory conditions do not exist, do not proceed until the conditions have 		      been rectified. Mounting surfaces should be flat, smooth and dry. Appropriate anchor shall be determined by installer to 		      support load of product weight under specified conditions. 

	3.02  PREPARATION

		A.  Measure and confirm specifications per shop drawing for installation area. Do not install if verification is negative.
		B.  Unpack all ABSORB panels and inspect. 
		C.  When more than one panel is adjacent, mock up panel array to ensure fit and finish. 
		D.  Ensure all panels are present.
	
	3.03  CONSTRUCTION

		A.  Coordination with other trades
			1.  Adjust panels as indicated on shop drawings to interface with all electrical apparatus, including outlets, 				     light fixtures and signage, HVAC system components, speakers, fire suppression systems including 				     sprinklers, switches, controls and piping, and other trade obstructions. Obstructions listed are for 					     reference and are not limited to above.   
			2.  ABSORB panels shall, in no circumstance, support the weight or interface of any other construction.

	3.03  INSTALLATION

		A.  Install panels according to architectural and shop drawings in accordance with manufacturer instructions. Use appropriate 		      mounting and anchoring.
		B.  Anchors must be set prior to installation.
		C.  Adhesives must be tacky prior to mounting.
		D.  All installations shall be conducted by experienced and qualified professional installers.
.

	3.04  ADJUSTMENT

		A.  After job installation is complete, adjust each panel to conform with specified drawings. If further adjustments are necessary, 		      take measures to ensure installation meets drawings.
			1.  Panel sides should be parallel with adjacent panels.
			2.  Adjust panels to ensure panels are level and parallel.
		B.  Remove and replace panels that do not meet or cannot be repaired to Architect or Owner's satisfaction. 

	3.05  CLEANING

		A.  Clean debris from installation from work site in an appropriate manner.
		B.  Vacuum dust and debris from panels with a soft brush attachment.
		C.  Clean dust and debris from panels with a slightly dampened cleaning cloth and wipe dry with a dry cleaning cloth. 
		D.  Remove all debris caused by this section from work site upon completion of installation. Crates, packaging, and associated 		      waste and debris shall be properly disposed of. 
		E.  Recycle materials when possible.


END OF SECTION
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